耗材供应一览表
	序号
	商品名称
	参数和商品类目
	品牌
	单位
	数量
	单价(元)
	金额
(元)

	1. 
	电池
	5号24粒7号16粒
	南孚（40粒）
	盒
	10
	78
	780

	2. 
	真空泵油
	4升UL19
	EDWARDS
	瓶
	4
	260
	1040

	3. 
	一次性手套
	XS、S蓝色耐用丁腈检查手套
	AMMEX爱马斯
	盒
	20
	50
	1000

	4. 
	棉拖鞋
	40、41、42、43码
	洁丽雅
	双
	20
	24
	480

	5. 
	EBSD样品台
	按图纸工厂定做
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	广州飞纳
	个
	4
	240
	960

	6. 
	EBSD样品台
	按图纸工厂定做
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	广州飞纳
	个
	4
	260
	1040

	7. 
	钨灯丝
	A054L
	蔡司
	根
	40
	240
	9600

	8. 
	钨灯丝
	A054
	蔡司
	根
	60
	220
	13200

	9. 
	导电胶
	双面碳导电胶8MM
	日本日新
	卷
	10
	350
	3500

	10. 
	样品盒
	12枚丁型台装
	广州飞纳
	个
	2
	180
	360

	11. 
	氮气
	99.9%
	蓝天气体
	瓶
	50
	180
	9000

	12. 
	液氮
	99.99%
	梅塞尔
	升
	400
	10
	4000

	13. 
	ZnO
	500g分析纯
	国药
	瓶
	2
	30
	60

	14. 
	CaCO3
	500g分析纯
	国药
	瓶
	2
	18
	36


	15. 
	水砂纸
	280#
	鹰牌
	张
	500
	0.52
	260

	16. 
	水砂纸
	320#
	鹰牌
	张
	500
	0.52
	260

	17. 
	变色硅胶
	2-4mm蓝色
	漠凡克
	瓶
	40
	10
	400

	18. 
	金相砂纸
	800#
	无锡牌
	盒
	5
	160
	800

	19. 
	金相砂纸
	1000#
	无锡牌
	盒
	5
	160
	800

	20. 
	金相砂纸
	1200#
	无锡牌
	盒
	5
	160
	800

	21. 
	金相砂纸
	2000#
	无锡牌
	盒
	5
	160
	800

	22. 
	凡士林
	500g
	天津致远化学试剂有限公司
	瓶
	10
	12
	120

	23. 
	镜头纸
	显微镜擦镜纸
	杭州双圈
	本
	50
	2
	100

	24. 
	无尘布
	5009
	净佰泰
	包
	100
	10
	1000

	25. 
	无水乙醇
	500ml
	安徽安特有限公司
	瓶
	50
	12
	600

	26. 
	脱脂棉
	长纤维
	鼎特，曹县和泰卫生材料
	包
	10
	24
	240

	27. 
	金相电吹风
	1800W  FH6276
	飞科
	把
	3
	50
	150

	28. 
	金刚石研磨膏
	5g,W2.5
	恒宇仪器
	支
	20
	5
	100

	29. 
	金刚石研磨膏
	5g，W2.5
	恒宇仪器
	支
	20
	5
	100

	30. 
	竹镊子
	15cm
	普瑞达办公用品
	个
	5
	5
	25

	31. 
	滴管烧杯
	50ml
	普瑞达办公用品
	个
	10
	5
	50

	32. 
	烧杯
	100ml
	普瑞达办公用品
	个
	5
	3
	15

	33. 
	量筒
	10ml
	普瑞达办公用品
	个
	2
	3
	6

	34. 
	量筒
	50ml
	普瑞达办公用品
	个
	2
	3
	6

	35. 
	烧杯
	50ml
	普瑞达办公用品
	个
	10
	3
	30

	36. 
	金相保护胶带
	宽度30mm，100米
	上海纳勒材料科研服务平台
	卷
	5
	80
	400

	37. 
	抛光膏
	0.5μm（350ml/瓶）
	精兢
	支
	5
	70
	350

	38. 
	抛光膏
	2.5μm（350ml/瓶）
	精兢
	支
	5
	70
	350

	39. 
	抛光膏
	1.5μm（350ml/瓶）
	精兢
	支
	5
	70
	350

	40. 
	双面胶带
	24mm
	京东得力
	卷
	20
	10
	200

	41. 
	链条油
	KOBY 85ml
	长城
	瓶
	2
	16
	32

	42. 
	Na2CO3
	500g，AR
	分析纯
	瓶
	2
	15
	30

	43. 
	口罩
	均码
	臻和亦康
	个
	200
	2.4
	480

	44. 
	帆布手套
	大、中、小码
	劳保
	双
	10
	5.4
	54

	45. 
	纱手套
	大、中、小码
	劳保
	双
	20
	5
	100

	46. 
	胶手套
	大、中、小码
	劳保
	双
	10
	12
	120

	47. 
	不锈钢桶
	50L
	普通
	个
	20
	15
	300

	48. 
	样品密封盒
	20*15*8cm
	乐扣乐扣
	个
	10
	20
	200

	49. 
	医用纱布
	棉质
	可孚
	包
	20
	8
	160

	50. 
	防冻液
	C3
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CZ Teplonosna a chladici kapalina vhodna k prenosu tepla nebo chladu na bézi vod’y.' Obsahuje ucinné inhibitory koroze a stabilizétory. Chréni kovové
materialy ze Zeleza, barevnych kol a jejich slitin (m,j. ocel, litina, mosaz) pred korozi. Preg’chgm vzniku a syt
Chrani okruh pred mikrobidIni kontaminaci (houbami, fasami a mikroorganismy). Nepouzivejte v materidlech z hliniku a zinku.

ku a usazeninam vodniho kamene. Nenapada pryZova tésnéni.
Névod k pouziti: CS COOLANT C3 pouzivejte jako naplii chladicich zafizen. Nikdy nemichejte s napinémi jinych vyrobcd, nefedte vodou nebo nedopliiujte jinym
Upozoméni: EUR 208 - Obsahuje 1,2-benzoisothiazol-3(2H)-on+ (<0,01 hm%). Mize vyvolat alergickou reakci. Pfi kontaktu s oééuina.kmttgi lvzglha:;ﬁrm
proudem isté vody min. 15 minut a vyhledat lékatskou pomoc. PFi kontaktu s kiizi: omyt zasazenou pokozku vodou a osetiit regeneracnim s o
poit: vyplachnout ista vodou, vypit cca 0,2 litru vody a vyhledat lékare. Skladovani: Skladujte v ptivodnim, dokonale uzavieném, neporusen: rytych,
suchych skladech. Chrafite pred
Minimélni trvanlivost: 60 mési
EN Heat transfer fluid

mrazem. Vyrobek pouzivejte pouze k uceliim uvedenym na této etiketé. Produkt a jeho obal Ize likvidovat béZnym zpusobem.
cli od data vyroby.
their alloys before corrosion, €S COO!

¢ S an 5 i i low metals and
used as coolant based on water. It contains corrosion inhibitors and stabilizators. Product protects materials from iron, yel

LANT (3 precedes and protects before production of incrusts and scales in system: It is compatible with common rubbers. It
protects system before microbial cof
Instruction manual: CS COOLANT

Pripravky. Pravidelné dopliwjte hladinu v okruhu. Vyménn Ihiita produktu ¢ini 24 mésicd. Je pouzitelny v rozmezi teplot +5 aZ 90 °C.

ntamination (fungi, algae and microorganisms). Do not use in contact with materials from aluminium and zinc.
C3 il to cooling machines. Never mix this product with other mixtures, do not dilute with water. Often please keep right volume
of your systems. Change period is 24 months, Product is used in temperature from +5 to 90 °C.
Warning: EUH 208 - Contains 1 2-benzoisothiazol-3(2H)-on+ (<0,01 wt.%)
immediate medical attention. In case of
medical attention. Storage conditions:

Skm contact: waSh with w’atel. “
mnsu‘“ed Dfodu(l and l.
W l p a [kag ¢ lspo

-May produce an allergic reaction. In case of efe contact: rinse with clean water and seek
swall’;wed: flush your mouth with water, drink about 0,2 L of water and seek mmedi::
Keepin sheltered, closed and tight original package, in t tures from 5 °C 1 40 °C. Protect before freeze! Used or
se under local laws. Minimal guarantee is 5 years from date of production.
e/Manufacturer: CLASSIC Oil 5.0, 0. Petka 343, Kladno. Ceska republika/Czech Republic - EU,
Wwwclassic-oil.cz, email: info@classic-oil.cz, tel. ¢ /n.; 040 608 185 185.
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	德国COOLANT
	升
	20
	80
	1600

	51. 
	锉刀8件套
	TK910-23C
	史丹利
	套
	1
	350
	350

	52. 
	金属清洗球
	7CM
	妙洁
	只
	20
	5
	100

	53. 
	一转三转换器

插座
	GN-934K
	公牛牌
	只
	10
	34
	340

	54. 
	实验塑料杯
	200ml
	佳乐祺
	包
	10
	12
	120

	55. 
	白色实验服
	长袖M、L、XL
	宝来逊
	件
	100
	48
	4800

	
	
	
	
	
	
	合计
	62154

	
	优惠后合计
	62000


供应商：湘潭市雨湖区致远科教设备经营部
